61 of 172
ZBasic Language Reference 54 ZX Microcontroller Family BasicX Compatibility Note In BasicX compatibility mode, enumerations may only be defined at the module level and qualification of an enumeration is not supported. Also, the values of enumeration members are only 8-bits wide in BasicX while they are 16-bit values in ZBasic. An alternate type conversion method is supported for compatibility reasons but is a bit awkward to use. For each defined enumeration, there is a special System Library conversion function just for that enumeration whose name is To<enum> where <enum> is replaced with the enumeration name. This special conversion function takes only one parameter, that being the value to convert. animal = ToMammal(3) One drawback to this conversion method is that there is no way to qualify the enumeration with the module name in which it is defined. It is recommended that all new applications use the CType() conversion function. 3.3 Serial Channels All of the ZX series devices support multiple serial channels. Channel 1 (COM1) is implemented using the USART hardware on the microcontroller chip. When the ZX begins running, COM1 is configured to run at 19.2K baud, 8 data bits, 1 stop bit. Your program can send and receive data using the default configuration by utilizing the console I/O routines like Console.Write(), Console.Read() and the related Debug.Print command. Some ZX devices have additional hardware-based serial channels but the remaining serial channels are implemented in software. This strategy allows a lot of flexibility in choosing which pins are used for transmission and reception but it also imposes a processing overhead on the system, even when characters are not being actively sent and received. Because of this, only one additional serial channel, COM3, is enabled for use by default. If you wish to utilize additional serial channels (COM4 to COM6) you must call the System Library routine ComChannels() to specify both the number of channels desired and the maximum baud rate that may be used. See the description of the ComChannels() routine in the ZBasic System Library Reference manual for more details. Since serial channels 3-6 rely on interrupts to achieve the necessary timing for serial I/O, if interrupts are disabled for a substantial fraction of the bit time (the inverse of the baud rate) the integrity of the transmitted or received characters may suffer. Typically, the maximum acceptable interrupt disable time is about 25% of the bit time of the fastest channel. If the fastest channel is running at 9600 baud, the interrupt disable time should be kept below 25µS or so. Many of the I/O routines that utilize Timer1 (e.g. PulseOut) disable interrupts in order to achieve precise timing. Those that do disable interrupts have a caveat to that effect in their respective descriptions in the ZBasic System Library Manual. See the descriptions of DefineCom(), OpenCom() and CloseCom() in the ZBasic System Library Manual for more details on setting up and using a serial channel. 3.4 Queues A queue is a fundamental data structure that is widely used in computer programs. Its primary distinguishing feature is that data items are extracted from the queue in the same order in which they were inserted. This is called first-in, first-out or FIFO order. One of the uses for a queue in ZBasic is as a temporary buffer for data going to and coming from one of the serial channels. Another common use is as a medium through which to pass data between tasks. The producer of the data puts data in the queue and the consumer of the data takes it from the queue. ZBasic queues are of a fixed length, that length being determined at the time that the queue is prepared for use using OpenQueue(). If the data producer inserts data faster than the consumer removes it, the