154 of 172
ZBasic Language Reference 147 ZX Microcontroller Family Reset Circuit You may also want to incorporate a reset button in your circuitry. If so, a normally open, momentary contact switch may be connected directly between pin 4 of the ZX and ground. If other circuitry in your application also needs the reset signal, you may want to isolate that circuitry from the ATN resets using a buffer gate or a diode. A suggested diode isolation circuit for the reset line is shown below. Reset Signal Isolation