153 of 172
ZBasic Language Reference 146 ZX Microcontroller Family Alternate Serial Interface Circuit #1 The first alternate above is similar to the circuitry used on the ZX-24 series. The advantage to this circuit is its simplicity. The disadvantage is that the voltage levels of the serial output signal do not meet the RS- 232 standard. Even so, most serial receivers are able to properly interpret the output signal. Note that if the inverters used have protection diodes on their inputs the external diodes shown are not necessary. The second alternate serial interface is shown in the diagram below. This circuit produces a serial output signal that meets the RS-232 standard by using the negative voltage on the receive line to provide a reference for the output level. Although the parts count is higher, the circuit uses inexpensive and non- critical components. Alternate Serial Interface Circuit #2