68 of 172
ZBasic Language Reference 61 ZX Microcontroller Family 3.8.1 CPU Registers ZX-24, ZX-40, and ZX-44 Registers The pre-defined CPU registers for the ZX-24, ZX40 and ZX-44 match those available on the ATmega32 CPU and all are Byte values. Discussion of the use of these registers is beyond the scope of this document. See the Atmel documentation for a full description. Also, be advised that modifying some of these registers may severely alter the behavior of the control program, possibly even rendering it inoperable. The register value may be accessed by using the register name, from the table below, prefixed by the keyword Register, e.g. Register.PortC. CPU Registers for mega32-based ZX Models ACSR EECR OCR1AL PORTD TCCR2 UBRRH ADCH EEDR OCR1BH SFIOR TCNT0 UBRRL ADCL GICR OCR1BL SPCR TCNT1H UCSRA ADCSRA GIFR OCR2 SPDR TCNT1L UCSRB ADMUX GIMSK OSCCAL SPH TCNT2 UCSRC ASSR ICR1H PINA SPL TIFR UDR DDRA ICR1L PINB SPMCR TIMSK WDTCR DDRB MCUCR PINC SPSR TWAR DDRC MCUSR PIND SREG TWBR DDRD MCUCSR PORTA TCCR0 TWCR EEARH OCR0 PORTB TCCR1A TWDR EEARL OCR1AH PORTC TCCR1B TWSR Some CPU registers are 16-bit values that have register names in the table above corresponding to the high and low bytes. For convenience of access, the following UnsignedInteger register names are available. When reading and writing to these registers, the control program ensures that the high and low bytes are accessed in the correct order as required by the CPU. Note that UBRR cannot be supported because the high and low bytes are not adjacent in the I/O address space. ADC EEAR ICR1 OCR1A OCR1B SP TCNT1 Because the ZX microcontrollers are implemented using a more powerful CPU, some registers available in BasicX don’t actually exist on the ZX CPU but there are equivalent registers. For compatibility, both the original register name and the actual register name are supported on similar ZX models. For new applications, the new register names should be used. BasicX Register New Register ADCSR ADCSRA GIMSK GICR MCUSR MCUCSR UBRR UBRRL¹ UCR UCSRB USR UCSRA Notes: ¹ The serial port baud rate control register is 16-bits wide in the mega32 CPU. The upper bits are referred to as UBRRH.