Page 185 of 229 Start Back Next End ZBasic Language Reference 175 ZBasic Microcontrollers Detailed Pin Descriptions Pin 25, Port D Bit 7 (ATmega) or Port E Bit 0 (ATxmega) This pin drives the red LED and may also be used for PWM generation based on Timer 2. See the Atmel documentation for more details on the latter function. Pin 26, Port D Bit 5 (ATmega) or Port D Bit 0 (ATxmega) This pin drives the green LED and may also be used for PWM generation based on Timer 1. See the Atmel documentation for more details on the latter function. Pin 27, Port D Bit 4 (ATmega) or Port D Bit 1 (ATxmega) This pin is the output point for the standard OutputCapture() routine. It may also be used for PWM generation based on Timer 1. See the Atmel documentation for more details on the latter function. SCK, MISO, MOSI These pins are the inputs and outputs for the SPI bus by which external SPI devices may be connected to the ZX-24 series device. CS For ZX devices with an on-board EEPROM, this pin is connected to the chip select pin for that device and to the SS (slave select) pin of the ATmega. For ZX devices without an on-board EEPROM, this pin is connected only to the SS (slave select) pin of the ATmega or ATxmega. Vcc, Reset, Gnd, CS These pins are used in the manufacturing and testing processes.