103 of 286
89 Get1WireData Type Subroutine Invocation Get1WireData(pin, data, count) Parameter Method Type Description pin ByVal Byte The pin to be used for 1-Wire I/O. data ByRef any type The variable to receive the bytes read. count ByVal Byte The number of bytes to read. Discussion This function retrieves 1 or more bytes (each LSB first) using the 1-Wire protocol and writes them to the given variable. To perform a 1-Wire operation, this function along with related 1-Wire routines must be used in the proper sequence. See the specifications of your 1-Wire device for more information. Caution If the variable provided has fewer bytes than the given count, subsequent memory locations will be altered, usually with undesirable consequences. Resource Usage This routine uses the I/O Timer and disables interrupts for about 100µS for each bit received. Example Dim ba(1 to 10) as Byte Call Get1WireData(12, ba, SizeOf(ba)) See Also Get1Wire, Get1WireByte, Put1Wire, Put1WireByte, Put1WireData, Reset1Wire