135 of 286
121 Valid Input Capture Pins ZX Models Timer1 Pin Timer3 Pin Timer4 Pin Timer5 Pin ZX-24, ZX-24a, ZX-24p, ZX-24n 12, D.6 - - - ZX-40, ZX-40a, ZX-40p, ZX-40n 20, D.6 - - - ZX-44, ZX-44a, ZX-44p, ZX-44n 15, D.6 - - - ZX-24e, ZX-24ae, ZX-24pe, ZX-24ne 14, D.6 - - - ZX-1281, ZX-1281n 29, D.4 9, E.7 - - ZX-1280, ZX-1280n 47, D.4 9, E.7 35, L.0 36, L.1 ZX-128e, ZX-128ne, ZX-1281e, ZX-1281ne 8, D.4 13, E.7 - - For native code devices, the table below gives the ISRs that may be loaded if your program uses InputCaptureEx(). If the compiler cannot determine which specific timer ISR is required by analyzing the parameters used, all listed ISRs will be included. ISRs Required Underlying CPU ISR Name mega644P Timer1_Capt, Timer1_OVF mega1281, mega128 Timer1_Capt, Timer1_OVF, Timer3_Capt, Timer3_OVF mega1280 Timer1_Capt, Timer1_OVF, Timer3_Capt, Timer3_OVF, Timer4_Capt, Timer4_OVF, Timer5_Capt, Timer5_OVF Example Dim pd(1 to 5) as UnsignedInteger Call PutPin(D.6, zxInputTriState) Call InputCaptureEx(D.6, pd, UBound(pd), 1) Compatibility This routine is not available in BasicX compatibility mode.