173 of 286
159 Output Capture Pin ZX Models Pin ZX-24, ZX-24a, ZX-24p, ZX-24n 27, D.4 ZX-40, ZX-40a, ZX-40p, ZX-40n 18, D.4 ZX-44, ZX-44a, ZX-44p, ZX-44n 13, D.4 ZX-24e, ZX-24ae, ZX-24pe, ZX-24ne 16, D.4 ZX-1281, ZX-1281n 25, B.6 ZX-1280, ZX-1280n 16, B.6 ZX-128e, ZX-1281e, ZX-128ne, ZX-1281ne 22, B.6 Compatibility Since the CPU runs at twice the rate as the BasicX CPU, the units of the pulse width are half as long. If you need to generate longer pulse widths, you may set the value of Register.TimerSpeed1 so that a slower clock rate is used. Also, the BasicX documentation indicates that if the I/O Timer is already in use, that use will be terminated and the waveform generation will be performed. See Also OutputCaptureEx()