188 of 286
174 Put1Wire Type Subroutine Invocation Put1Wire(pin, value) Parameter Method Type Description pin ByVal Byte The pin to be used for 1-Wire I/O. value ByVal Byte The bit value to write. Discussion This routine sends the LSB of the given value using the 1-Wire protocol. To perform a 1-Wire operation, this function along with related 1-Wire routines must be used in the proper sequence. See the specifications of your 1-Wire device for more information. Resource Usage This routine uses the I/O Timer and disables interrupts for about 100µS. Example Call Put1Wire(12, 1) See Also Get1Wire, Get1WireByte, Get1WireData, Put1WireByte, Put1WireData, Reset1Wire