177 of 286
163 Pause Type Subroutine Invocation Pause(time) Parameter Method Type Description time ByVal Single or int16 The amount of time to pause, in seconds (Single) or Timer 0 ticks (int16) Discussion This routine suspends execution of the current task for approximately the period of time specified. No other task is allowed to run during the pause period. The resolution of the time period is approximately 4.34µS with a maximum pause time of about 284mS. Note that the accuracy of the pause may be affected by the time required for the processor to service interrupts (RTC, serial channel, etc.). Also note that the resolution of the pause is similar to the minimum execution time for user instructions. This means that timing using Pause() calls of less than 20 to 50 units or so will be affected significantly by the succeeding instructions. This routine should be used instead of Sleep() or Delay() when higher resolution timing is required or you don’t want a task switch to occur. If you need longer pauses than can be produced by this routine, you can implement them using Register.RTCStopWatch. Example Do Call PutPin(12, 0) Call Pause(0.010) ' a 10 millisecond delay Call PutPin(12, 1) Call Pause(2304) ' a 10 millisecond delay Loop This loop produces a square wave signal on pin 12 at approximately 50Hz (with some jitter due to handling interrupts). Compatibility This routine is not available in BasicX compatibility mode. See Also Delay, DelayUntilClockTick, Sleep, WaitForInterval