252 of 307
ZBasic System Library 242 ZX Microcontroller Family Normally, the data pin will be driven high or low according to the data bits being shifted out. For compatibility with certain data bus interfaces, the flags parameter bit 3 can be used to specify that the data pin should be put in high impedance input mode when outputting a one bit and actively pulled to ground for a zero bit. In this mode, an external pullup resistor will need to be used to obtain a voltage level corresponding to a logic one. For reference purposes, the ShiftOut() routine is roughly equivalent to ShiftOutEx(dpin, cpin, bitCnt, Shl(CInt(val), 8), &H04, 74). Resource Usage This subroutine uses the I/O Timer if the flags parameter has bit 2 on. If the I/O Timer is already in use, the subroutine returns immediately. No other use of this resource should be attempted while the shifting is in progress. Interrupts are disabled during the shifting process. However, RTC ticks are accumulated during the shifting process so the RTC should not lose time. Compatibility This function is not available in BasicX compatibility mode. See Also ShiftIn, ShiftInEx, ShiftOut