86 of 307
ZBasic System Library 76 ZX Microcontroller Family This call prepares channel 1 for transmit-only using pin 12, non-inverted logic, MSB-first operation. Compatibility This subroutine is not available on ZX models that are based on the ATmega32 processor (e.g. the ZX- 24). The second form is only available on native mode devices. Neither form is available in BasicX compatibility mode. See Also CloseX10, OpenX10, StatusX10