55 of 318
ZBasic System Library 45 ZX Microcontroller Family ClosePWM8 Type Subroutine Invocation ClosePWM8(channel) ClosePWM8(channel, status) Parameter Method Type Description channel ByVal Byte The 8-bit PWM channel to close. status ByRef Boolean A variable to receive the status code. Discussion This subroutine terminates the PWM signal generation on the specified 8-bit channel and all other PWM channels associated with the same 8-bit timer. The resulting state of the output pins for the affected channels is indeterminate. If your application requires a specific output state, it is recommended that you call PutPin() to set the desired state prior to calling ClosePWM8(). The status parameter, if supplied, receives a value to indicate success or failure of the call. A side effect of a successful ClosePWM8() call is that the timer busy flag for the associated timer (e.g. Register.Timer2Busy) will be set to False indicating that the timer may be used for other purposes. Example Call ClosePWM8(1) ' terminate PWM on channel 1 (and channel 2) Compatibility This subroutine is not available in BasicX compatibility mode nor is it available on ATxmega-based ZX devices. See Also OpenPWM8, PWM8