200 of 323
ZBasic System Library 190 ZX Microcontroller Family Output Capture Pin ZX Models Pin ZX-24, ZX-24a, ZX-24p, ZX-24n, ZX-24r, ZX-24s 27, D.4 ZX-40, ZX-40a, ZX-40p, ZX-40n, ZX-40r, ZX-40s 18, D.4 ZX-44, ZX-44a, ZX-44p, ZX-44n, ZX-44r, ZX-44s 13, D.4 ZX-24e, ZX-24ae, ZX-24ne, ZX-24pe, ZX-24nu, ZX-24pu, ZX-24ru, ZX-24su 16, D.4 ZX-328n, ZX-328l, ZX-32n, ZX-32l 16, B.2 ZX-1281, ZX-1281n 25, B.6 ZX-1280, ZX-1280n 16, B.6 ZX-24x, ZX-32a4, ZX-24xu 11, C.1 ZX-128a1 16, C.1 ZX-128e, ZX-1281e, ZX-128ne, ZX-1281ne 22, B.6 ZX-328nu 13, B.2 Compatibility For devices running at 14.7MHz, since the CPU runs at twice the rate as the BasicX CPU, the units of the pulse width are half as long. If you need to generate longer pulse widths, you may set the value of Register.TimerSpeed1 so that a slower clock rate is used. Also, the BasicX documentation indicates that if the I/O Timer is already in use, that use will be terminated and the waveform generation will be performed. See Also OutputCaptureEx