316 of 323
ZBasic System Library 306 ZX Microcontroller Family on what it can determine from analysis of the various invocations. If the compiler is unable to determine which specific ISR is require, all those listed will be included. ISRs Required Underlying CPU Int Type ISR Name mega644P, mega1284P External Interrupt Pin Change Interrupt Analog Comparator INT0, INT1, INT2 PCINT0, PCINT1, PCINT2, PCINT3 Analog_Comp mega328P External Interrupt Pin Change Interrupt Analog Comparator INT0, INT1 PCINT0, PCINT1, PCINT2 Analog_Comp mega128 External Interrupt Analog Comparator INT0, INT1, INT2, INT3, INT4, INT5, INT6, INT7 Analog_Comp mega1281 External Interrupt Pin Change Interrupt Analog Comparator INT0, INT1, INT2, INT3, INT4, INT5, INT6, INT7 PCINT0, PCINT1, PCINT2 Analog_Comp mega1280 External Interrupt Pin Change Interrupt Analog Comparator INT0, INT1, INT2, INT3, INT4, INT5, INT6, INT7 PCINT0, PCINT1, PCINT2 Analog_Comp xmega32A4 Pin Change Interrupt Analog Comparator PORTA_INT0, PORTA_INT1 PORTB_INT0, PORTB_INT1, PORTC_INT0, PORTC_INT1 PORTD_INT0, PORTD_INT1, PORTE_INT0, PORTE_INT1 ACA_AC0, ACA_AC1, ACA_ACW xmega128A1 Pin Change Interrupt Analog Comparator PORTA_INT0, PORTA_INT1, PORTB_INT0, PORTB_INT1, PORTC_INT0, PORTC_INT1, PORTD_INT0, PORTD_INT1, PORTE_INT0, PORTE_INT1, PORTF_INT0, PORTF_INT1, PORTH_INT0, PORTH_INT1, PORTJ_INT0, PORTJ_INT1, PORTK_INT0, PORTK_INT1, PORTQ_INT0, PORTQ_INT1 ACA_AC0, ACA_AC1, ACA_ACW, ACB_AC0, ACB_AC1, ACB_ACW Compatibility The second parameter is not supported in BasicX compatibility mode. The built-in constant zxPinChange is not available in BasicX. It is not known if the capability is supported or not.