192 of 323
ZBasic System Library 182 ZX Microcontroller Family OpenSPI Type Subroutine Invocation OpenSPI(channel, flags, csPin) OpenSPI(channel, flags, csPin, rxDelay) Parameter Method Type Description channel ByVal Byte The SPI channel to open (1-4). flags ByVal integral Flags controlling the SPI communication. csPin ByVal Byte The pin for the chip select signal to the device. rxDelay ByVal Byte The delay time prior to each received byte. Discussion This subroutine prepares an SPI channel for use as a master. By default, the hardware SPI controller is used to implement the SPI protocol but on some devices, a bit-bang implementation can be enabled (see DefineSPI). Four channels are supported, numbered 1 through 4. It does not matter if the particular channel has been previously opened. The flags parameter specifies the characteristics of the SPI communication as shown in the table below. They must be set to be compatible with the device with which you want to communicate. See the table below for details. The csPin parameter specifies the pin number that you wish to control the device’s chip select input. The pin will be made an output and set to the inactive state (as specified by bit 6 of the flags parameter). Note that any general purpose I/O pin of the device may be used as the slave select pin except for the SS pin of the device. The shaded entries in the table below do not apply to the software SPI implementation. SPI Channel Control Bits Function Hex Value Binary Value Bit Rate f/4 &H00 xx xx xx 00 Bit Rate f/16 &H01 xx xx xx 01 Bit Rate f/64 &H02 xx xx xx 10 Bit Rate f/128 &H03 xx xx xx 11 Clock Phase False &H00 xx xx x0 xx Clock Phase True &H04 xx xx x1 xx Clock Low at Idle &H00 xx xx 0x xx Clock High at Idle &H08 xx xx 1x xx Use Hardware SPI &H00 xx x0 xx xx Use Software SPI &H10 xx x1 xx xx Bit Order – MSB first &H00 xx 0x xx xx Bit Order – LSB first &H20 xx 1x xx xx Active Low Chip Select &H00 x0 xx xx xx Active High Chip Select &H40 x1 xx xx xx Double Speed &H80 1x xx xx xx The remaining bits are currently undefined but they may be employed in the future. Because of this possibility, the undefined flag bits should be zero. Bits 3 and 2 taken together specify the SPI mode 0-3, e.g. xx xx 00 xx specifies mode 0. When using the hardware SPI controller, if the Double Speed bit is set, the SPI channel will run at twice the frequency specified by the two low order flag bits. The value of f for the bit rate selector is the CPU frequency (typically 14.7456MHz). For the software SPI implementation, the number of cycles per bit is a minimum of about 50 so the implementation runs at full speed with either the f/4 or f/16 speed settings.