223 of 323
ZBasic System Library 213 ZX Microcontroller Family Examples Dim acc as Byte Call PutDAC(12, 0.5, acc) Call PutDAC(12, 128, acc, 5) Compatibility In BasicX compatibility mode, the dacValue parameter may only be specified using a Single value. Also, the fourth parameter is not supported. Resource Usage This routine disables interrupts for about 200µS during the generation process. Interrupts are reenabled between each successive cycle. See Also DAC, DACPin, OpenDAC