92 of 323
ZBasic System Library 82 ZX Microcontroller Family DelayUntilClockTick Type Subroutine Invocation DelayUntilClockTick() Discussion This routine suspends the current task until at least the next tick of the RTC. The actual delay depends on what other tasks actually do that may run in the interim. It is possible that the task will be suspended indefinitely. If no other tasks are ready to run, the actual delay could be between 0 and 1.95ms. This routine is exactly equivalent to Sleep(1). See Also Delay, Pause, Sleep