23 of 323
ZBasic System Library 13 ZX Microcontroller Family PORTE_INT1 ACA_AC0 ACA_AC1 ACA_ACW ACB_AC0 ACB_AC1 ACB_ACW PORTE_INT1 PORTF_INT0 PORTF_INT1 PORTH_INT0 PORTH_INT1 PORTJ_INT0 PORTJ_INT1 PORTK_INT0 PORTK_INT1 PORTQ_INT0 PORTQ_INT1 ACA_AC0 ACA_AC1 ACA_ACW ACB_AC0 ACB_AC1 ACB_ACW Timers ZX devices have three or more timers, depending on the underlying CPU type, that are used for various purposes. One of the timers is used to implement the real time clock (RTC), another is used for the software-based serial ports and a third timer is used to provide the precise timing required for certain I/O routines. The specific timer that is used for a particular function varies depending on the underlying CPU type as shown in the table below. Timer Usage by CPU Type Underlying CPU RTC I/O Serial 16-bit PWM InputCapture OutputCapture mega32, mega328P, mega644, mega644P Timer0 Timer1 Timer2 Timer1 Timer1 Timer1 mega1284P Timer0 Timer3 Timer2 Timer1 Timer3 Timer1 Timer3 Timer1 Timer3 mega128 Timer0 Timer1 Timer2 Timer1 Timer3 Timer1 Timer3 Timer1 Timer3 mega1281 Timer2 Timer4 Timer0 Timer1 Timer3 Timer1 Timer3 Timer1 Timer3 mega1280 Timer2 Timer4 Timer0 Timer1 Timer3 Timer4 Timer5 Timer1 Timer3 Timer4 Timer5 Timer1 Timer3 Timer4 Timer5 xmega32A4 TimerC1 TimerE0 TimerD1 TimerC0 TimerD0 TimerD1 TimerE0 TimerC0 TimerD0 TimerD1 TimerE0 TimerC0 TimerD0 TimerD1 TimerE0 xmega128A1 TimerC1 TimerF1 TimerD1 TimerC0 TimerD0 TimerD1 TimerE0 TimerE1 TimerF0 TimerF1 TimerC0 TimerD0 TimerD1 TimerE0 TimerE1 TimerF0 TimerF1 TimerC0 TimerD0 TimerD1 TimerE0 TimerE1 TimerF0 TimerF1 The RTC Timer is programmed to generate an interrupt that is used to update the RTC and to trigger task switching. Because its role is so central, the RTC Timer cannot be used for any other purpose. The I/O Timer is used by several I/O related routines as explained in more detail below. The Serial Timer is used to generate interrupts to implement the timing required for serial channels Com3 to Com6. If none of the channels 3-6 is open, the Serial Port Timer can be used for other purposes in your program. Timers are