116 of 323
ZBasic System Library 106 ZX Microcontroller Family GetADC (function form) Type Function returning Integer Invocation GetADC(pin) Parameter Method Type Description pin ByVal Byte The pin from which to read an analog voltage. Discussion This function performs an analog-to-digital conversion of the voltage present on the specified pin which must be one of the analog port pins (see the table below). The return value will be a 10-bit digital approximation of the input voltage with a range from zero to the reference voltage (see below). The return value represents the measured voltage voltage according to the formula V ref * adcVal / FS where V ref is the reference voltage, adcVal is the value returned by GetADC(), and FS is 1024 for mega- based devices and 4096 for xmega-based devices. You must make the specified pin an input before calling this routine. For ATmega-based devices, the conversion is performed using the AVcc reference voltage (connected internally to Vcc on the ZX-24, ZX-24a, ZX-24p, ZX-24n, ZX-24r, ZX-24s, ZX-24e, ZX-24ae, ZX-24ne, ZX- 24pe, ZX-24nu, ZX-24pu, ZX-24ru, ZX-24su, ZX-328nu, ZX-128e, ZX-128ne, ZX-1281e and ZX-1281ne). For ATxmega-based devices, the conversion is performed using a reference voltage of Vcc/1.6. Resource Usage Only analog port pins may be used to perform an analog-to-digital conversion. The analog port pins vary depending on the ZX model and some ZX models have more analog input pins available. Also, on some devices (e.g. ZX-32n, ZX-32l and ZX-328nu) some of the pins are dedicated analog inputs; having no digital functions. Analog Ports and Pins ZX Models Port Pins Port Pins ZX-24, ZX-24a, ZX-24p, ZX-24n, ZX-24r, ZX-24s PortA 13-20 - - ZX-40, ZX-40a, ZX-40p, ZX-40n, ZX-40r, ZX-40s PortA 33-40 - - ZX-44, ZX-44a, ZX-44p, ZX-44n, ZX-44r, ZX-44s PortA 30-37 - - ZX-328n, ZX-328l PortC 23-28 - - ZX-32n, ZX-32l PortC 23-28, 19, 22 - - ZX-1281, ZX-1281n PortF 54-61 - - ZX-1280, ZX-1280n PortF 90-97 PortK 82-89 ZX-24x PortA 13-20 PortB 7-9 ZX-32a4 PortA 40-44, 1-3 PortB 4-7 ZX-128a1 PortA 95-100, 1, 2 PortB 5-12 ZX-24e, ZX-24ae, ZX-24ne, ZX-24pe, ZX-24nu, ZX-24pu, ZX-24ru, ZX-24su PortA 29-36 - - ZX-24xu PortA 29-36 PortB 25-28 ZX-128e, ZX-128ne, ZX-1281e, ZX-1281ne PortF 29-36 - - ZX-328nu PortC 17-24 - - Most ZX processors contain a single analog-to-digital converter thus allowing only one conversion to be performed at a time. The conversion process takes approximately 220uS during which time the calling task will be awaiting conversion completion.