216 of 323
ZBasic System Library 206 ZX Microcontroller Family PulseIn (function form) Type Function returning Integer Invocation PulseIn(pin, level) Parameter Method Type Description pin ByVal Byte The pin on a pulse width will be measured. level ByVal Byte The expected pulse logic value (high = 1). Discussion This routine waits for the input pin to be in the idle state (the opposite of that specified by the level parameter), waits for it to change to the specified logic level and then measures the time that it stays at that level. The width of the pulse is returned by the function, the units of which are 2 times the I/O Timer period. At the default I/O Timer clock period of 0.54µS, the returned value has units of 1.08µS. The pin is made an input if it is not already so. If the awaited logic transition never occurs or if the pulse width exceeds the maximum representable width the returned value will be zero. The timing resolution may be adjusted using Register.TimerSpeed2. Note that for compatibility with BasicX, the timing resolution is one half of the period of the selected I/O Timer frequency. Resource Usage This routine uses the I/O Timer and interrupts are disabled during the pulse measurement. However, RTC ticks will be accumulated during the pulse measurement and the RTC will be updated when the process is complete. Example Dim width as Integer i = PulseIn(12, 1) ' measure a positive pulse Compatibility The BasicX implementation does not support adjustable timing resolution.