Page 203 of 346 Start Back Next End ZBasic System Library 191 ZBasic Microcontrollers The status parameter, if supplied, receives a value to indicate success or failure of the call. Example Call OpenDAC(1, &H01) ' prepare for DAC output using AVcc reference Call DAC(1, 300) ' set the DAC level to 300/4095*AVcc Compatibility This subroutine is only available for xmega target devices and is not available in BasicX compatibility mode. See Also CloseDAC, DAC