Page 334 of 346 Start Back Next End ZBasic System Library 322 ZBasic Microcontrollers ValueS Type Subroutine Invocation ValueS(str, val, flag) Parameter Method Type Description str ByVal String The string from which to extract a floating point value. val ByRef Single The variable to receive the value. flag ByRef Boolean The variable to receive a success indicator. Discussion This routine converts a character representation of a floating pointer number, contained in the str parameter, to a Single value returned in the val parameter. If the string is in an acceptable format, the flag parameter is set to True. Otherwise, the flag parameter is set to False and the val parameter will be 0.0. The string may contain any number of leading and/or trailing spaces. The value itself may consist solely of decimal digits or may have a leading plus or minus sign. The value may include a decimal point, with or without preceding digits. However, there must be a digit either preceding the decimal point or following it, or both. Optionally, there may be a multiplier value consisting of the letter E (upper or lower case), optionally followed by a plus or minus sign, followed by one or more digits. Note that the range of acceptable input is wider than that for real values in ZBasic statements. If the provided string has the proper format but represents a value that is too large or too small to be represented as a Single, the result will be invalid but no such indication will be given. Examples of floating point numbers accepted by ValueS() are: .30103 3.14159 -200. 1e05 +6.02E+23 123 See Also ValueI, ValueL