Page 201 of 346 Start Back Next End ZBasic System Library 189 ZBasic Microcontrollers Resource Usage See the resource usage sub-section UARTs for information on which UART is assigned to each available serial channel, the transmit and receive pins, and the ISRs utilized for native mode devices. The software-based serial channels are implemented using the Serial Timer. See the resource usage sub-section Timers for information on which timer is used for a particular target device Compatibility In BasicX, the supported channel numbers are 1 to 3, depending on the particular target chip. Also, BasicX doesn’t support the use of zero to indicate that no queue is being supplied. See Also ComChannels, CloseCom, ControlCom, DefineCom, StatusCom