Page 268 of 346 Start Back Next End ZBasic System Library 256 ZBasic Microcontrollers 37 Awaiting pin change event Q1. The task resumes as if the pin change event had occurred. 38 Awaiting analog comp. A0. The task resumes as if the analog event had occurred. 39 Awaiting analog comp. A1. The task resumes as if the analog event had occurred. 40 Awaiting analog comp. AW. The task resumes as if the analog event had occurred. 41 Awaiting analog comp. B0. The task resumes as if the analog event had occurred. 42 Awaiting analog comp. B1. The task resumes as if the analog event had occurred. 43 Awaiting analog comp. BW. The task resumes as if the analog event had occurred. 254 Task exiting. None, exiting tasks can’t be resumed. 255 Terminated. None, halted tasks can’t be resumed. If this routine is invoked using an array other than one that is or was being used for a task stack the result is undefined. See the section on Task Management in the ZBasic Reference Manual for additional information regarding task management. Compatibility This routine is not available in BasicX compatibility. See Also ExitTask, RunTask, StatusTask, WaitForInterrupt