Page 235 of 346 Start Back Next End ZBasic System Library 223 ZBasic Microcontrollers Put1Wire Type Subroutine Invocation Put1Wire(pin, value) Parameter Method Type Description pin ByVal Byte The pin to be used for 1-Wire I/O. value ByVal Byte The bit value to write. Discussion This routine sends the LSB of the given value using the 1-Wire protocol. To perform a 1-Wire operation, this function along with related 1-Wire routines must be used in the proper sequence. See the specifications of your 1-Wire device for more information. Resource Usage This routine uses the I/O Timer and disables interrupts for about 100µS. Example Call Put1Wire(12, 1) See Also Get1Wire, Get1WireByte, Get1WireData, Put1WireByte, Put1WireData, Reset1Wire