Page 31 of 346 Start Back Next End ZBasic System Library 19 ZBasic Microcontrollers for the duration of the input capture operation. Note that an input capture cannot be used at the same time as an output capture operation involving the same timer. For native code ZX devices and all generic target devices, at least two ISRs will be automatically provided by the compiler to facilitate the input capture operation corresponding to the capture interrupt and the timer overflow interrupt. The names of the interrupt vectors are related to the timer being used. For example, for Timer1 the names are Timer1_Capt and Timer1_OVF. Note that if the compiler cannot determine at compile time which timer will be used, the capture and timer overflow ISRs for all possible timers will be included in the application. Valid Input Capture Pins for ZX Devices ZX Device Timer Pin ZX-24, ZX-24a, ZX-24p, ZX-24n Timer1 12, D.6* ZX-40, ZX-40a, ZX-40p, ZX-40n Timer1 20, D.6* ZX-44, ZX-44a, ZX-44p, ZX-44n Timer1 15, D.6* ZX-24r, ZX-24s Timer1 Timer3 12, D.6* B.5 ZX-40r, ZX-40s, ZX-40t Timer1 Timer3 20, D.6* 6, B.5 ZX-44r, ZX-44s, ZX-44t Timer1 Timer3 15, D.6* 1, B.5 ZX-24e, ZX-24ae, ZX-24ne, ZX-24pe, ZX-24nu, ZX-24pu Timer1 14, D.6* ZX-24ru, ZX-24su Timer1 Timer3 14, D.6* 23, B.5 ZX-328n, ZX-328l Timer1 14 B.0* ZX-32n, ZX-32l Timer1 12 B.0* ZX-1281, ZX-1281n Timer1 Timer3 29, D.4* 9, E.7 ZX-1280, ZX-1280n Timer1 Timer3 Timer4 Timer5 47, D.4* 9, E.7 35, L.0 36, L.1 ZX-24x TimerC0 TimerD0 TimerE0 12, C.0* 26, D.0 25, E.0 ZX-32a4 TimerC0 TimerD0 TimerE0 10, C.0* 20, D.0 28, E.0 ZX-128a1 TimerC0 TimerD0 TimerE0 TimerE1 TimerF0 TimerF1 15, C.0* 25, D.0 35, E.0 39, E.4 45, F.0 49, F.4 ZX-128e, ZX-128ne, ZX-1281e, ZX-1281ne Timer1 Timer3 8, D.4* 13, E.7 ZX-328nu Timer1 11, B.0* ZX-24xu TimerC0 TimerD0 TimerE0 12, C.0* 20, D.0 24, E.0 Valid Input Capture Pins for Generic Target Devices Underlying CPU Type Pkg. Timer Pin tiny24, tiny24A, tiny44, tiny44A, tiny84 P14 Timer1 6, A.7* Q20 Timer1 15, A.7* tiny48, tiny88 P28 Timer1 14, B.0* T28 Timer1 10, B.0* T32 Timer1 12, B.0*