Page 118 of 346 Start Back Next End ZBasic System Library 106 ZBasic Microcontrollers DelayUntilClockTick Type Subroutine Invocation DelayUntilClockTick() Discussion This routine suspends the current task until at least the next tick of the RTC. The actual delay depends on what other tasks actually do that may run in the interim. It is possible that the task will be suspended indefinitely. If no other tasks are ready to run, the actual delay could be between 0 and 1 RTC tick. This routine is exactly equivalent to Sleep(1). However, the RTC must be enabled in your application in order to use this subroutine. See Also Delay, Pause, Sleep