Page 266 of 346 Start Back Next End ZBasic System Library 254 ZBasic Microcontrollers ResetX10 Type Subroutine Invocation ResetX10(chan, mask) Parameter Method Type Description chan ByVal Byte The X-10 communication channel of interest. mask ByVal Byte A mask value indicating which state flags to clear. Discussion Calling this routine will clear some of the flags that are returned by the StatusX10() function. The mask parameter should contain a value with a 1 in the bit positions corresponding to the state flags that you want to be cleared. Note that only a subset of the flags can be reset; asserted bits in the other bit positions are ignored. See the description of StatusX10() for more information. Compatibility This subroutine is supported only for native mode devices and is not available in BasicX compatibility mode. See Also StatusX10