Page 236 of 346 Start Back Next End ZBasic System Library 224 ZBasic Microcontrollers Put1WireByte Type Subroutine Invocation Put1WireByte(pin, value) Parameter Method Type Description pin ByVal Byte The pin to be used for 1-Wire I/O. value ByVal Byte The value to write. Discussion This routine sends a byte (LSB first) using the 1-Wire protocol. To perform a 1-Wire operation, this function along with related 1-Wire routines must be used in the proper sequence. See the specifications of your 1-Wire device for more information. Example Call Put1WireByte(12, &H55) Resource Usage This routine uses the I/O Timer and disables interrupts for about 100µS for each bit sent. Compatibility This routine is not available in BasicX compatibility mode. See Also Get1Wire, Get1WireByte, Get1WireData, Put1Wire, Put1WireData, Reset1Wire