Page 30 of 346 Start Back Next End ZBasic System Library 18 ZBasic Microcontrollers 8-bit PWM Timers, Channels and Pins for Generic Target Devices Target Devices Pkg. Timer Chan. Pin Chan. Pin tiny48, tiny88 all - tiny24, tiny24A, tiny44, tiny44A, tiny84 P14 Timer0 1 5, B.2 2 6, A.7 Q20 1 14, B.2 2 15, A.7 tiny87, tiny167 S20 Timer0 1 3, A.2 T32 1 31, A.2 tiny2313, tiny2313A, tiny4313 P20 Timer0 1 14, B.2 2 9, D.5 Q20 Timer0 1 7, B.2 2 12, D.5 mega8, mega8A P28 Timer2 1 17, B.3 T28 1 13, B.3 T32 1 15, B.3 mega48, mega48A, mega48P, mega48PA,mega88, mega88A, mega88P, mega88PA, mega168, mega168A, mega168P, mega168PA, mega328, mega328P P28 Timer2 1 17, B.3 2 5, D.3 T28 1 13, B.3 2 1, D.3 T32 1 15, B.3 2 1, D.3 mega16, mega16A, mega32, mega32A P40 Timer2 1 21, D.7 T44 Timer2 1 16, D.7 mega644, mega644A, mega164A, mega164P, mega164PA, mega324P, mega324PA, mega644P, mega644PA, mega1284P P40 Timer2 1 21, D.7 2 20, D.6 T44 Timer2 1 16, D.7 2 15, D.6 mega64, mega64A, mega128, mega128A, AT90CAN32, AT90CAN64, AT90CAN128 T64 Timer0 1 17, B.7 mega1281, mega2561 T64 Timer0 1 17, B.7 2 1, G.5 AT90USB646, AT90USB647, AT90USB1286, AT90USB1287 T64 Timer0 1 17, B.7 2 25, D.0 mega640, mega1280, mega2560 T100 Timer0 1 26, B.7 2 1, G.5 mega8U2, mega16U2, mega32U2, AT90USB82, AT90USB162 T32 Timer0 1 21, B.7 6 6, B.0 mega16U4, mega32U4 T44 Timer4 1 3 32, C.7 27, D.7 2 30, B.6 mega8515 P40 Timer0 1 1, B.0 T44 1 40, B.0 L44 1 2, B.0 mega8535 P40 Timer2 1 21, D.7 T44 1 16, D.7 L44 1 22, D.7 mega161, mega162 P40 Timer2 1 2, B.1 T44 1 41, B.1 mega163, mega323 P40 Timer2 1 21, D.7 T44 1 16, D.7 mega165, mega165A, mega165P, mega165PA, mega325, mega325P, mega645, mega645A, mega645P, mega169, mega169A, mega169P, mega169PA, mega329, mega329P, mega329PA, mega649, mega649A, mega649P T64 Timer2 1 17, B.7 mega3250, mega3250P, mega6450, mega6450A, mega6450P, T100 mega3290, mega3290P, mega6490, mega6490A, mega6490P Timer2 1 26, B.7 all xmega all - Input Capture Timers The tables below give the set of valid pins for the InputCaptureEx subroutine and also indicate (with an asterisk) the default pin used by the InputCapture subroutine. When an input capture operation has been started successfully, the corresponding timer busy flag (e.g. Register.Timer1Busy) will be set True