Page 39 of 346 Start Back Next End ZBasic System Library 27 ZBasic Microcontrollers ZX-24xu 29-36, 25-28 ZX-328nu 17-24 Analog Input Pins for Generic Target Devices Target Device Pkg. Analog Inputs tiny2313, tiny2313A, tiny4313, mega8515, mega161, mega162, mega8U2, mega16U2, mega32U2, AT90USB82, AT90USB162 all - tiny24, tiny24A, tiny44, tiny44A, tiny84 P14 6-13 Q20 1-5, 15, 16, 20 tiny48, tiny88 P28 23-28 T28 19-24 T32 23-28, 19, 22 tiny87, tiny167 S20 1-4, 7-10, 12, 13 T32 29-31, 3, 9-12, 15, 18, 19 mega48, mega48A, mega48P, mega48PA, mega8, mega8A, mega88, mega88A, mega88P, mega88PA, mega168, mega168A, mega168P, mega168PA, mega328, mega328P P28 23-28 T28 23-28, 19, 22 T32 23-28, 19, 22 mega16, mega16A, mega164A, mega164P, mega164PA, mega32, mega32A, mega324P, mega324PA, mega644, mega644A, mega644P, mega644PA, mega1284P P40 33-40 T44 40-47 mega64, mega64A, mega128, mega128A, mega1281, mega2561, AT90CAN32, AT90CAN64, AT90CAN128 T64 54-61 mega640, mega1280, mega2560 T100 82-89, 90-97 mega16U4, mega32U4 T44 36-41 mega8535, mega163, mega323 P40 33-40 T44 30-37 L44 36-43 mega165, mega165A, mega165P, mega165PA, mega325, mega325P, mega645, mega645A, mega645P, mega169, mega169A, mega169P, mega169PA, mega329, mega329P, mega329PA, mega649, mega649A, mega649P T64 54-61 mega3250, mega3250P, mega6450, mega6450A, mega6450P, mega3290, mega3290P, mega6490, mega6490A, mega6490P T100 90-97 AT90USB646, AT90USB647, AT90USB1286, AT90USB1287 T64 54-61 xmega16a4, xmega32a4 T44 40-44, 1-3, 4-7 xmega16d4, xmega32d4 T44 40-44, 1-3 xmega64a3, xmega128a3, xmega256a3, xmega256a3b T64 62-64, 1-5, 6-13 xmega64d3, xmega128d3, xmega192d3, xmega256d3 T64 62-64, 1-5 xmega64a1, xmega128a1 T100 95-100, 1-2, 5-12 Digital-to-Analog Converters The table below indicates the available channels and the corresponding DAC hardware used. Supported DAC Channels for ZX Devices ZX Devices DACB DACA ZX-24x Chan 1, Pin 8 Chan 2, Pin 9 - ZX-32a4 Chan 1, Pin 6 (B.2) Chan 2, Pin 7 (B.3) - ZX-128a1 Chan 1, Pin 7 (B.2) Chan 2, Pin 8 (B.3) Chan 3, Pin 97 (A.2) Chan 4, Pin 98 (A.3) ZX-24xu Chan 1, Pin 26 (B.2) -