Page 264 of 346 Start Back Next End ZBasic System Library 252 ZBasic Microcontrollers Reset1Wire Type Function returning Byte Invocation Reset1Wire(pin) Parameter Method Type Description pin ByVal Byte The pin to be used for 1-Wire I/O. Discussion This function generates a reset signal on the given pin using the 1-Wire protocol. The return value is the “presence” bit sent by the attached 1-Wire device(s), if any. It will be zero if a 1-Wire device responded, 1 otherwise. To perform a 1-Wire operation, this function along with related 1-Wire routines must be used in the proper sequence. See the specifications of your 1-Wire device for more information. Resource Usage This routine uses the I/O Timer and disables interrupts for approximately 1mS. Example Dim b as Byte b = Reset1Wire(12) Compatibility This routine is not available in BasicX compatibility mode. See Also Get1Wire, Get1WireByte, Get1WireData, Put1Wire, Put1WireByte, Put1WireData