Page 240 of 346 Start Back Next End ZBasic System Library 228 ZBasic Microcontrollers Examples Dim acc as Byte Call PutDAC(12, 0.5, acc) Call PutDAC(12, 128, acc, 5) Compatibility In BasicX compatibility mode, the dacValue parameter may only be specified using a Single value. Also, the fourth parameter is not supported. Resource Usage This routine disables interrupts for about 3000 CPU cycles (200µS at 14.7MHz) during the generation process. Interrupts are reenabled between each successive cycle. See Also DAC, DACPin, OpenDAC