Page 111 of 346 Start Back Next End ZBasic System Library 99 ZBasic Microcontrollers Compatibility This function is not available in BasicX compatibility mode; you must use DefineCom3(). Additionally, BasicX does not support 8-bit plus parity modes nor does it support the “Ignore Parity” mode. Furthermore, in BasicX characters received in 7-bit/no parity mode are aligned toward the MSB while in this implementation they are properly aligned toward the LSB. For mega32-based ZX devices (e.g. the ZX-24), the ability to define the characteristics of Com1 is not supported nor is half-duplex bussed mode supported. Specifying the same pin for rx and tx on these devices will produce undefined results. See Also ComChannels, ControlCom, OpenCom, StatusCom