Page 324 of 346 Start Back Next End ZBasic System Library 312 ZBasic Microcontrollers Timer Type Function returning Single Invocation Timer() Discussion This function returns the current RTC time represented as the number of seconds since midnight with a best-case resolution of 1/F_RTC_TICK. Note that Register.RTCTick gives you the equivalent information albeit in the form of a 32-bit value representing the number of RTC ticks (increments of 1/F_RTC_TICK) since midnight. Depending on your needs, one or the other may be more efficient to use. Compatibility This subroutine is not available if the RTC is not enabled in your application.