Page 48 of 346 Start Back Next End ZBasic System Library 36 ZBasic Microcontrollers heap size for a particular device and application. The tables below give the Program Memory page size for ZX devices and generic target devices. Program Memory Page Size for ZX Devices ZX Device Page Size ZX-24, ZX-24a, ZX-24p, ZX-40, ZX-40a, ZX-40p, ZX-44, ZX-44a, ZX-44p, ZX-24e, ZX-24ae, ZX-24pe, ZX-24pu n/a ZX-24n, ZX-40n, ZX-44n, ZX-24ne, ZX-24nu 256 ZX-24r, ZX-24s, ZX-40r, ZX-40s, ZX-40t, ZX-44r, ZX-44s, ZX-44t, ZX-24ru, ZX-24su 256 ZX-328n, ZX-328l, ZX-32n, ZX-32l, ZX-328nu 128 ZX-1281, ZX-1281n, ZX-1280, ZX-1280n 256 ZX-24x, ZX-32a4, ZX-24xu 256 ZX-128a1 512 ZX-128e, ZX-128ne, ZX-1281e, ZX-1281ne 256 Program Memory Page Size for Generic Target Devices Target Device Page Size tiny2313, tiny2313A, tiny24, tiny24A 32 tiny4313, tiny44, tiny44A, tiny84, tiny48, tiny88 64 tiny87, tiny167 128 mega48, mega48A, mega48P, mega48PA, mega8, mega8A, mega88, mega88A, mega88P, mega88PA 64 mega168, mega168A, mega168P, mega168PA, mega328, mega328P, mega16, mega16A, mega164A, mega164P, mega164PA, mega32, mega32A, mega324P, mega324PA 128 mega644, mega644A, mega644P, mega644PA, mega1284P, mega64, mega64A, mega128, mega128A, mega1281, mega2561, mega640, mega1280, mega2560 256 AT90CAN32, AT90CAN64, AT90CAN128 256 mega8U2 64 mega16U2, mega32U2 128 mega16U4, mega32U4 256 mega8515, mega8535 64 mega161, mega162, mega163, mega323 128 mega165, mega165A, mega165P, mega165PA, mega325, mega325P, mega169, mega169A, mega169P, mega169PA, mega329, mega329P, mega329PA, mega3250, mega3250P, mega3290, mega3290P 128 mega645, mega645A, mega645P, mega649, mega649A, mega649P, mega6450, mega6450A, mega6450P, mega6490, mega6490A, mega6490P 256 AT90USB82, AT90USB162 128 AT90USB646, AT90USB647, AT90USB1286, AT90USB1287 256 xmega64a1, xmega16a4, xmega32a4, xmega16d4, xmega32d4, xmega64a3, xmega64d3, 256 xmega128a1, xmega128a3, xmega256a3, xmega256a3b, xmega128d3, xmega192d3, xmega256d3 512