Page 91 of 346 Start Back Next End ZBasic System Library 79 ZBasic Microcontrollers ControlCom Type Subroutine Invocation ControlCom(chan, rxFlowPin, txFlowPin) ControlCom(chan, rxFlowPin, txFlowPin, flags) Parameter Method Type Description chan ByVal Byte The serial channel of interest. rxFlowPin ByVal Byte The pin to use for receive flow control. txFlowPin ByVal Byte The pin to use for transmit flow control. flags ByVal Byte Flag bits controlling the sense of the flow control lines. Discussion This subroutine sets a flow control pin for the receive side and/or transmit side of a serial channel. Either or both of the second and third parameters may be zero indicating that that type of flow control is not desired. If the fourth parameter is not specified, it defaults to the value zero indicating that the flow control pins should be active high. If the fourth parameter is specified, the bits of its value have the meaning given in the table below. Flag Parameter Values Value Meaning &H01 The receive flow control pin should be active low. &H02 The transmit flow control pin should be active low. The remaining bits are currently undefined but may be used in the future. For compatibility with new functionality that may be added in the future, the unused bits should always be zero. If a receive flow control pin is specified, the pin will be made an output and placed in the active state. This indicates to the sender that the ZX is ready to accept serial data. When the channel’s receive queue is nearly full (two bytes of space left), the receive flow control pin will be set to the inactive state indicating to the sender that data transmission should be temporarily suspended. When additional space becomes available in the receive queue (at least three bytes), the receive flow control pin will be set back to the active state. If a transmit flow control pin is specified, the pin will be made an input. Before sending data, the ZX will check the state of the transmit flow control pin and, if it is at the inactive level, no data will be sent. Note that the input is checked periodically and transmission will resume if the transmit flow control pin is in the active state when sampled. The current state of the flow control signals is part of the value returned by StatusCom(). It is important to note that a receive queue that is too small is likely to result in a deadlock since there will never be enough free space to activate the flow control signal. Also, when a channel is closed the flow control settings for the channel are cleared. For that reason, it is recommended that the call to ControlCom() be made, if desired, some time after a channel is opened and before it is closed. Compatibility This subroutine is not available on ZX devices based on the mega32 (e.g. ZX-24). Moreover it is not available in BasicX compatibility mode. See Also CloseCom, ComChannels, DefineCom, OpenCom, StatusCom