19 of 172
ZBasic Language Reference 12 ZX Microcontroller Family Examples Option StringSize 25 Option StringSize Default Option Strict Option Strict [On | Off | Default] Default: Off This option directive, supported for BasicX compatibility, enables or disables so-called “strict syntax checking”. You can enable strict mode by using Option Strict by itself or by including the keyword On. You disable strict syntax checking by using Option Strict Off. Specifying Option Strict Default sets the option to the default for the currently selected language. The implications of strict syntax checking are noted in the description of each affected element but a summary of the effects is given here. - the loop index variable of a For loop has restrictions on lifetime, visibility and accessibility - logical operators like Not, And and Or may not be used with signed integral data types This option has local scope, i.e., it only affects compilation of the module in which the option appears. Example Option Strict Off Option TargetDevice Option TargetDevice <device-name> Default: ZX24 Due to differences between the various members of the ZX- series, the compiler needs to know for which device it should compile the code. This allows it to generate the correct code for the intended device. At present, the supported values for <device-name> are given in the table below. The device names are not case sensitive. ZX24 ZX24a ZX24p ZX24n ZX40 ZX40a ZX40p ZX40n ZX44 ZX44a ZX44p ZX44n ZX1281 ZX1281n ZX1280 ZX1280n ZX328n ZX328l ZX28n ZX28l ZX24e ZX24ae ZX24pe ZX24ne ZX128e ZX128ne ZX1281e ZX1281ne ZX328nu Example Option TargetDevice ZX24a Option TargetCPU Option TargetCPU <CPU-type> Default: ZX24 This option is deprecated, use Option TargetDevice instead.