163 of 208
ZBasic Language Reference 155 ZX Microcontroller Family Public Volatile CtrlFClr as Byte Public Volatile CtrlFSet as Byte Public Volatile CtrlGClr as Byte Public Volatile CtrlGSet as Byte Public Volatile IntFlags as Byte Public Volatile unused2(1 to 2) as Byte Public Volatile Temp as Byte Public Volatile unused3(1 to 16) as Byte Public Volatile Cnt as UnsignedInteger Public Volatile unused4(1 to 4) as Byte Public Volatile Per as UnsignedInteger Public Volatile CCA as UnsignedInteger Public Volatile CCB as UnsignedInteger Public Volatile unused5(1 to 10) as Byte Public Volatile PerBuf as UnsignedInteger Public Volatile CCABuf as UnsignedInteger Public Volatile CCBBuf as UnsignedInteger End Structure ' For accessing USARTs: Structure USART_t Public Volatile Data as Byte Public Volatile Status as Byte Public Volatile unused1 as Byte Public Volatile CtrlA as Byte Public Volatile CtrlB as Byte Public Volatile CtrlC as Byte Public Volatile BaudCtrlA as Byte Public Volatile BaudCtrlB as Byte End Structure