97 of 208
ZBasic Language Reference 89 ZX Microcontroller Family Public ttime as MyTime Private isCurrent as Boolean End Structure Sub Main() Dim ts as MyTimeStamp Call GetTimeStamp(ts.tdate.year, ts.tdate.month, ts.tdate.day, _ ts.ttime.hour, ts.ttime.minute, ts.ttime.seconds) End Sub The example above illustrates how members of an instance of a structure are referenced. The variable ts is an instance of the MyTimeStamp structure. A member is referenced by appending the member name to the variable name, separating them with a period. For members that are structures, members of the subordinate structure are referred to similarly. No spaces are allowed in this construction. In cases where a variable or a member is an array, the index list directly follows the variable/member name, preceding the period. Structure foo Dim b as Byte Dim ai(1 to 10) as Integer Dim ts(1 to 4) as MyTimeStamp End Structure Dim yr as UnsignedInteger Dim i as Integer Dim f as foo Dim b as Byte i = f.ai(b) yr = f.ts(3).tdate.year The address of a member of a variable that is a structure may be obtained by appending the .DataAddress property identifier to the reference or by using the MemAddress() function. Dim addr as UnsignedInteger addr = ts.tdate.DataAddress addr = MemAddressU(ts.tdate) Structures may be used in Alias and Based variable definitions. However, in these cases the structures may not contain members that are any of the string types. Structures may be passed to subroutines and functions either by reference or by value. If a structure is passed by value, the structure will be read-only within the procedure. A variable that is a structure may be assigned to another variable that is the same type of structure using the standard assignment operator. In most cases, the compiler produces code to implement the copy operation using a simple memory-to-memory copy operation. However, in cases where the structure contains one or more members that are of the allocated string type (or has members that are structures which have such members), the compiler uses a special copy procedure that ensures the correct result. Moreover, two variables that are the same type of structure may be compared for equality or inequality using the standard comparison operators, = and <>. The equality/inequality test is implemented using a byte-by-byte comparison of the content of two structures. If one or more members of the structure are the BoundedString type, the byte-by-byte comparision may result in a False value even though the strings are identical. This is because the currently-unused portion of the string store may contain byte values that are different between the two instances being compared. Similarly, comparison of structures containing allocated strings, while allowed, is not recommended because of the likelihood of resulting in false negatives.