Page 63 of 229 Start Back Next End ZBasic Language Reference 53 ZBasic Microcontrollers Stack Usage by Parameter Type and Passing Method Actual Parameter Type Pass By Value Pass By Reference Boolean, Byte 1 2 Bit, Nibble 1 2² Integer, UnsignedInteger, Enum 2 2 Long, UnsignedLong, Single 4 2 String¹, structure 2 2 Array, any type n/a 2 Notes: ¹ Persistent strings, Program Memory strings and strings returned by functions all require 4 bytes of temporary data space (local to the caller) plus the 2-byte reference when passed to a routine other than a System Library routine. ² Sub-byte types like Bit and Nibble may only be passed by reference if they are byte aligned. See Section 3.24.1 for details. 2.15 Program and Data Item Properties Most data items, whether located in RAM, Persistent Memory or Program Memory have an associated property called DataAddress that evaluates to the address of the data item. The DataAddress property is applied to a data item by appending it to the data item’s name with a period separating them as illustrated by the example below. Example Dim b as Byte Dim addr as UnsignedInteger Sub Main() addr = b.DataAddress End Sub The DataAddress property can be applied to arrays and structures as well. When used with arrays it is best to append it after the array indices, if any. For most data items, the type of the DataAddress property is UnsignedInteger. However, for compatibility with GetProgMem() and other routines related to Program Memory, the type of the DataAddress property for Program Memory data items is Long. Along similar lines, subroutines and functions have an associated property called CodeAddress whose type is Long. The CodeAddress property is employed in a similar manner as the DataAddress property is as shown by the example below. Of course, use of the CodeAddress property of a subroutine is not limited to the code in the subroutine itself. It can be applied to any subroutine or function that is visible to the code. In short, if you can invoke the subroutine or function, you can also get its address via the CodeAddress property. Example Dim addr as Long Sub Main() addr = Main.CodeAddress End Sub It should be noted that for native mode devices, the CodeAddress property returns a word address instead of the usual byte address. In most cases, this fact is transparent but it should be kept in mind for special circumstances such as passing the address of a procedure to GetProgMem() for example. One advantage of this anomaly is that procedure addresses for ZBasic devices containing up to 128K of Program Memory may be represented in 16-bit data items on native mode devices.