223 of 307
ZBasic System Library 213 ZX Microcontroller Family DegToRad() facilitate the conversion between the two systems. Depending on optimization settings, if the parameter supplied to this function is known to be constant at compile time, the compiler will convert the value at compile time. Otherwise, code is generated to perform the conversion (multiplication by a conversion factor) at run time. Example Dim f as Single Dim theta as Single ' the angle in degrees theta = RadToDeg(Asin(f)) Compatibility This function is not available in BasicX compatibility mode. See Also