230 of 307
ZBasic System Library 220 ZX Microcontroller Family RamPokeWord Type Subroutine Invocation RamPokeWord(value, address) Parameter Method Type Description value ByVal int16 The value to write to RAM. address ByVal int16 The RAM address to which to write. Discussion This routine will write the given value to the two bytes at the specified RAM address, least significant byte first. Caution Modifying user variables in this way may cause your program to malfunction. Writing to areas of RAM used by the system may cause your program to malfunction. Example Dim u as UnsignedInteger Call RamPokeWord(&H55aa, MemAddress(u)) Compatibility This routine is not available in BasicX compatibility mode. See Also RamPoke, RamPokeDword