132 of 307
ZBasic System Library 122 ZX Microcontroller Family GetTimestamp Type Subroutine Invocation GetTimestamp(year, month, day, hour, minute, seconds) Parameter Method Type Description year ByRef int16 The variable in which to place the year value (1999-2177). month ByRef Byte The variable in which to place the month value (1-12). day ByRef Byte The variable in which to place the day value (1-31). hour ByRef Byte The variable in which to place the hour value (0-23). minute ByRef Byte The variable in which to place the minutes value (0-59). seconds ByRef Single The variable in which to place the seconds value. Discussion This routine decomposes the value of Register.RTCDay and Register.RTCTick into year, month, day, hour, minute and second components. See GetDate() and GetTime() for more details.