285 of 307
ZBasic System Library 275 ZX Microcontroller Family Timer Type Function returning Single Invocation Timer() Discussion This function returns the current RTC time represented as the number of seconds since midnight with a best-case resolution of 1.95ms. Note that Register.RTCTick gives you the equivalent information albeit in the form of a 32-bit value representing the number of 1.95ms ticks since midnight. Depending on your needs, one or the other may be more efficient to use.