118 of 307
ZBasic System Library 108 ZX Microcontroller Family GetEEPROM Type Subroutine Invocation GetEEPROM(addr, var, count) Parameter Method Type Description addr ByVal Long The Program Memory address from which to begin reading. var ByRef any type The variable in which to place the data read. count ByVal int16 The number of bytes to read. Discussion This routine is provided for compatibility with BasicX. The more aptly named GetProgMem() should be used by new applications. See Also GetProgMem, PutProgMem