86 of 318
ZBasic System Library 76 ZX Microcontroller Family DefineCom3 Type Subroutine Invocation DefineCom3(rxPin, txPin, flags) Parameter Method Type Description rxPin ByVal Byte The pin which will serve as the receive line. txPin ByVal Byte The pin which will serve as the transmit line. flags ByVal Byte Configuration flags. See the discussion below. Discussion This routine is provided solely for BasicX compatibility. It is equivalent to using Call DefineCom(3, rxPin, txPin, flags). See the DefineCom() routine for more information.