244 of 323
ZBasic System Library 234 ZX Microcontroller Family RamPokeDword Type Subroutine Invocation RamPokeDword(value, address) Parameter Method Type Description value ByVal any 32-bit The value to write to RAM. address ByVal int16 The RAM address to which to write. Discussion This routine will write the given value to the four bytes at the specified RAM address, least significant byte first. Caution Modifying user variables in this way may cause your program to malfunction. Writing to areas of RAM used by the system may cause your program to malfunction. Example Dim ul as UnsignedLong Call RamPokeDword(&H117355aa, MemAddress(ul)) Call RamPokeDword(&H117355aa, ul.DataAddress) Compatibility This routine is not available in BasicX compatibility mode. See Also RamPoke, RamPokeWord