Page 242 of 346 Start Back Next End ZBasic System Library 230 ZBasic Microcontrollers PutEEPROM Type Subroutine Invocation PutEEPROM(addr, var, count) Parameter Method Type Description addr ByVal Long The Program Memory address at which to begin writing. var ByRef any type The variable from which the data to be written will be taken. count ByVal int16 The number of bytes to write. Discussion This routine is provided for compatibility with BasicX. The more aptly named PutProgMem() should be used by new applications. See Also GetProgMem, PutProgMem